

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | | |
| **Quotation for 36m2 Foam Cement House** | | | | | | | | | | | |
| **PRICE DETAIL** | | | | | | | | | | | |
| NO. | PART | DESCRIPTION | | QUANTITY | | UNIT | |  | |  | | |
| **Cement House Main Body** | | | | | | | | | | | |
| 1 | Mainbody | Cement House Main Body | | 36 | | M2 | |  | |  | | |
| **Doors and Windows** | | | | | | | | | | | |
| 2 | Doors | Steel Security Door for Entrance（D1） | | 1 | | SET | |  | |  | | |
| Composite Wood Door for Bedroom(D2) | | 3 | | SET | |  | |  | | |
| Windows | Aluminum Sliding Window W1 | | 4 | | PCS | |  | |  | | |
| Aluminum Sliding Window W2 | | 1 | | PCS | |  | |  | | |
| **Total Doors and Windows Price** | | | | | | | | |  | | |
| **Decoration Materials** | | | | | | | | | | | |
| 3 | Floor Decoration | Cermic Tile | | 96 | | PCS | |  | |  | | |
| **Total Decoration Price** | | | | | | | | |  | | |
|  | | | | | | | | | | | |
| DESCRIPTION | | | QUANTITY | | UNIT | |  | |  | | |
| 4 | 40'HQ Qingdao Port Inland Shipping and Port Charges | | | 2 | | Container | |  | |  | | |
| Total Inland Shipping and Port Charges | | | | | | | | |  | | |
|  | | | | | | | | |  | | |
|  | **House Design Draw** | | | | | | | | | | | |
| 5 |  | | | | | | | | | | | |
| 6 | Payment Terms | 100% T/T before loading | | | | | | | | | | |
| 7 | Validity of Quotation | 15 days | | | | | | | | | | |
| 8 | Shipping | By Sea, the Loading Port, Qingdao, China | | | | | | | | | | |
| 9 | Packing | 1\*40'HQGP containers can load 2 unit of this house with all above | | | | | | | | | | |
| 10 | Size | SPEC: 6.6m\*5.4m\*2.8m | | | | | | | | | | |
| **Materials List** | | | | | | | | | | | |
| **No.** | **PART** | **First Part (Main Part of House)** | | **Material** | | **Specification** | | **Quantity** | | **Unit** | **Picture** | |
| 1 | Mainbody Panel | 94mm External Wall Panel | | Foamed Cement Panel | | 8mm Fiber Cement Board on two surface; 78mm thickness Foam Cement Core; Build-in Steel Structure | | 73.1 | | M2 |  | |
| 2 | 94mm Internal Wall Panel | | 35.3 | | M2 |
| 3 | 94mm Roof Panel | | 44.9 | | M2 |
| 4 | Structure to Fix Pane | Square Tube(Using for Basement,Use Expansion Bolt to fix it,then Wall Panel sit on the Square Tube) | | Square Tube | | 30mm\*30mm\*2mm | | 36.6 | | M |  | |
| 5 | Square Tube (Using for Ring Beam to strength the Whole Steel Structure) | | Square Tube | | 30mm\*30mm\*2mm | | 25.8 | | M |  | |



|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 6 | Panel Gap Painting | Plaster for External Wall | White | 11.5m2 Use One Bag | 10 | BAG |  |
| 7 | Plaster for Internal Wall | 12 | BAG |
| 8 | Sealing Tape for Gap Fixing | White | Standard | 23 | PCS |  |
| 9 | Undercoat | Standard | Standard | 27 | KG |  |
| 10 | `Beam | A-Beam | Hot Galvanized Steel 5400m(Length) | L50\*50\*3 | 2 | PCS |  |
| 11 | Roof | Glazed tile | Galvanize Steel | 828mm\*0.5mm | 57.6 | M |  |
| 12 | Ridge tile | 0.5mm | 7.5 | M |  |
| **NO.** | **PART** | **Second Part (Doors and Windows)** | **Material** | **Specification** | **Quantity** | **Unit** | **Picture** |
| 1 | Doors | Steel Security Door for Entrance | Steel | 960mm\*2050mm (W\*L) | 1 | SET |  |
| 2 | Composite Wood Door for Bedroom | Wood | 860mm\*2050mm (W\*L) | 2 | SET |  |
| 3 | Aluminum Alloy Door | Aluminum Alloy | 750mm\*2050mm (W\*L) | 1 | SET |  |
| 4 | Windows | Aluminum Sliding Window(white and single glass) | Aluminum Alloy | 1140mm\*1300mm (L\*W) | 6 | PCS |  |
| 6 | 1140mm\*900mm (L\*W) | 1 | PCS |
| 7 | 540mm\*900mm (L\*W) | 1 | PCS |
| **NO.** | **PART** | **Third Part (Decoration Materials)** | **Material** | **Specification** | **Quantity** | **Unit** | **Picture** |
| 1 | Floor Decoration | Ceramic Tiles for Internal Floor | Ceramic Tile | 600mm\*600mm\*10 mm  (L\*W\*T) | 96 | PCS |  |
| Note: This offer for current materials market; The Price is not including installation expenses | | | | | | | |
|  | | | | | | | |
| **2018-6-19** | | | | | | | |