All-In-One Solar LED Street Light 2018



|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Model No. | Photos | Description | Packing Information | EXW Price(3 Years Warranty) Lifepo4 Battery |
| **AL-220** |  | 1. Material: Aluminum alloy
2. Solar Panel:18V25W (high efficiency monocrystalline silicon)

LED Brand: 20W High Brightness Bridgelux LED1. Output Lumen: 2000-2200lm

Batterylithium battery 12V/10AH (Lifepo4 Lithium)1. Mounting Height: 3-4m
2. Work time: 12 hours and 5-7 rain days
3. Work temperature: -25℃~+65℃

Protection Grade: IP651. Certificates: CE/ROHS/TUV
 | Packing Size: 600\*415\*135mm Net Weight: 5.5KGGross Weight: 6.5KG Carton Packing: 1 set / ctn Container Loading:20GP: 800 pcs40GP: 1660 pcs | **US$190.00** |
| **AL-230** | 1. Material:Aluminum alloy
2. Solar Panel:18V30W (high efficiency monocrystalline silicon)
3. LED Brand: 30W High Brightness Bridgelux LED

Output Lumen: 3000-3300lm1. Batterylithium battery 12V/12AH (Lifepo4 Lithium)
2. Mounting Height: 5-6m
3. Work time: 12 hours and 5-7 rain days

Work temperature:-25℃~+65℃1. Protection Grade: IP65
2. Certificates: CE/ROHS/TUV
 | Packing Size: 660\*415\*135mm Net Weight: 6.0KGGross Weight: 7.0KGCarton Packing: 1 set / ctn Container Loading:20GP: 730 pcs40GP:1510 pcs | **US$240.00** |
| **AL-240** | 1. Material:Aluminum alloy
2. Solar Panel:18V36W (high efficiency monocrystalline silicon)
3. LED Brand: 40W High Brightness Bridgelux LED

Output Lumen: 4000-4400lm1. Batterylithium battery 12V/15AH (Lifepo4 Lithium)

Mounting Height: 6-7m1. Work time: 12 hours and 5-7 rain days

Work temperature:-25℃~+65℃1. Protection Grade: IP65
2. Certificates: CE/ROHS/TUV
 | Packing Size: 750\*415\*220mm Net Weight: 9.8KGGross Weight:11.0KGCarton Packing: 1 set / ctn Container Loading:20GP: 395 pcs40GP: 825 pcs | **US$278.00** |
| **AL-250** | Material:Aluminum alloy1. Solar Panel:18V40W (high efficiency monocrystalline silicon)

LED Brand: 50W High Brightness Bridgelux LED1. Output Lumen: 5000-5500lm
2. Batterylithium battery 12/18AH (Lifepo4 Lithium)

Mounting Height: 6-7m1. Work time: 12 hours and 5-7 rain days
2. Work temperature: -25℃~+65℃

Protection Grade: IP651. Certificates: CE/ROHS/TUV
 | Packing Size: 880\*415\*230mmNet Weight: 11.0KGGross Weight: 12.0KG Carton Packing: 1 set / ctn Container Loading:20GP: 320 pcs40GP: 666 pcs | **US$332.00** |
| **AL-260** | Material:Aluminum alloy1. Solar Panel:18V45W (high efficiency monocrystalline silicon)
2. LED Brand: 60W High Brightness Bridgelux LED

Output Lumen: 6000-6600lm1. Batterylithium battery 12V/21AH (Lifepo4 Lithium)
2. Mounting Height: 7-8m

Work time: 12 hours and 5-7 rain days1. Work temperature: -25℃~+65℃
2. Protection Grade: IP65
3. Certificates: CE/ROHS/TUV
 | Packing Size: 880\*415\*230mmNet Weight: 11.5KG Gross Weight: 12.5KGCarton Packing: 1 set / ctnContainer Loading: 20GP: 320 pcs40GP: 666 pcs | **US$360.00** |
| **AL-270** | Material:Aluminum alloy1. Solar Panel:18V55W (high efficiency monocrystalline silicon)

LED Brand: 70W High Brightness Bridgelux LED1. Output Lumen: 7000-7700lm
2. Batterylithium battery 12V/24AH (Lifepo4 Lithium)

Mounting Height: 8-9m1. Work time: 12 hours and 5-7 rain days

Work temperature:-25℃~+65℃1. Protection Grade: IP65
2. Certificates: CE/ROHS/TUV
 | Packing Size: 1100\*415\*230mmNet Weight: 12.5KGGross Weight: 15.0KG Carton Packing: 1 set / ctn Container Loading:20GP: 270 pcs40GP: 560 pcs | **US$395.00** |
| **AL-280** | Material:Aluminum alloy1. Solar Panel:18V60W (high efficiency monocrystalline silicon)

LED Brand: 80W High Brightness Bridgelux LED1. Output Lumen: 8000-8800lm

Batterylithium battery 12V/27AH (Lifepo4 Lithium)1. Mounting Height: 8-9m
2. Work time: 12 hours and 5-7 rain days

Work temperature:-25℃~+65℃1. Protection Grade: IP65
2. Certificates: CE/ROHS/TUV
 | Packing Size: 1100\*415\*230mmNet Weight: 13.0KGGross Weight: 15.5KG Carton Packing: 1 set / ctn Container Loading:20GP: 270 pcs40GP: 560 pcs | **US$420.00** |

# RRMARK:

## 1: Above prices are based on EXW. Valid date to 31st Aug 2018. 2: 1~2 days for samples, 5~7 days for standard orders add 100% plus courier fee.

3: The solar controller and battery are built inside of light head.

4 : The controller needs extra 5.0USD, 10pcs of solar led street light need 1pc controller 5: Lighting mode can be changed by remote controller.