All-In-One Solar LED Street Light 2018



|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Model No. | Photos | Description | Packing Information | EXW Price  (3 Years Warranty) Lifepo4 Battery |
| **AL-220** |  | 1. Material: Aluminum alloy 2. Solar Panel:18V25W (high efficiency monocrystalline silicon)  LED Brand: 20W High Brightness Bridgelux LED  1. Output Lumen: 2000-2200lm  Batterylithium battery 12V/10AH (Lifepo4 Lithium)  1. Mounting Height: 3-4m 2. Work time: 12 hours and 5-7 rain days 3. Work temperature: -25℃~+65℃  Protection Grade: IP65  1. Certificates: CE/ROHS/TUV | Packing Size: 600\*415\*135mm Net Weight: 5.5KG  Gross Weight: 6.5KG Carton Packing: 1 set / ctn Container Loading:  20GP: 800 pcs  40GP: 1660 pcs | **US$190.00** |
| **AL-230** | 1. Material:Aluminum alloy 2. Solar Panel:18V30W (high efficiency monocrystalline silicon) 3. LED Brand: 30W High Brightness Bridgelux LED  Output Lumen: 3000-3300lm  1. Batterylithium battery 12V/12AH (Lifepo4 Lithium) 2. Mounting Height: 5-6m 3. Work time: 12 hours and 5-7 rain days  Work temperature:-25℃~+65℃  1. Protection Grade: IP65 2. Certificates: CE/ROHS/TUV | Packing Size: 660\*415\*135mm Net Weight: 6.0KG  Gross Weight: 7.0KG  Carton Packing: 1 set / ctn Container Loading:  20GP: 730 pcs  40GP:1510 pcs | **US$240.00** |
| **AL-240** | 1. Material:Aluminum alloy 2. Solar Panel:18V36W (high efficiency monocrystalline silicon) 3. LED Brand: 40W High Brightness Bridgelux LED  Output Lumen: 4000-4400lm  1. Batterylithium battery 12V/15AH (Lifepo4 Lithium)  Mounting Height: 6-7m  1. Work time: 12 hours and 5-7 rain days  Work temperature:-25℃~+65℃  1. Protection Grade: IP65 2. Certificates: CE/ROHS/TUV | Packing Size: 750\*415\*220mm Net Weight: 9.8KG  Gross Weight:11.0KG  Carton Packing: 1 set / ctn Container Loading:  20GP: 395 pcs  40GP: 825 pcs | **US$278.00** |
| **AL-250** | Material:Aluminum alloy  1. Solar Panel:18V40W (high efficiency monocrystalline silicon)  LED Brand: 50W High Brightness Bridgelux LED  1. Output Lumen: 5000-5500lm 2. Batterylithium battery 12/18AH (Lifepo4 Lithium)  Mounting Height: 6-7m  1. Work time: 12 hours and 5-7 rain days 2. Work temperature: -25℃~+65℃  Protection Grade: IP65  1. Certificates: CE/ROHS/TUV | Packing Size: 880\*415\*230mm  Net Weight: 11.0KG  Gross Weight: 12.0KG Carton Packing: 1 set / ctn Container Loading:  20GP: 320 pcs  40GP: 666 pcs | **US$332.00** |
| **AL-260** | Material:Aluminum alloy  1. Solar Panel:18V45W (high efficiency monocrystalline silicon) 2. LED Brand: 60W High Brightness Bridgelux LED  Output Lumen: 6000-6600lm  1. Batterylithium battery 12V/21AH (Lifepo4 Lithium) 2. Mounting Height: 7-8m  Work time: 12 hours and 5-7 rain days  1. Work temperature: -25℃~+65℃ 2. Protection Grade: IP65 3. Certificates: CE/ROHS/TUV | Packing Size: 880\*415\*230mm  Net Weight: 11.5KG Gross Weight: 12.5KG  Carton Packing: 1 set / ctn  Container Loading: 20GP: 320 pcs  40GP: 666 pcs | **US$360.00** |
| **AL-270** | Material:Aluminum alloy  1. Solar Panel:18V55W (high efficiency monocrystalline silicon)  LED Brand: 70W High Brightness Bridgelux LED  1. Output Lumen: 7000-7700lm 2. Batterylithium battery 12V/24AH (Lifepo4 Lithium)  Mounting Height: 8-9m  1. Work time: 12 hours and 5-7 rain days  Work temperature:-25℃~+65℃  1. Protection Grade: IP65 2. Certificates: CE/ROHS/TUV | Packing Size: 1100\*415\*230mm  Net Weight: 12.5KG  Gross Weight: 15.0KG Carton Packing: 1 set / ctn Container Loading:  20GP: 270 pcs  40GP: 560 pcs | **US$395.00** |
| **AL-280** | Material:Aluminum alloy  1. Solar Panel:18V60W (high efficiency monocrystalline silicon)  LED Brand: 80W High Brightness Bridgelux LED  1. Output Lumen: 8000-8800lm  Batterylithium battery 12V/27AH (Lifepo4 Lithium)  1. Mounting Height: 8-9m 2. Work time: 12 hours and 5-7 rain days  Work temperature:-25℃~+65℃  1. Protection Grade: IP65 2. Certificates: CE/ROHS/TUV | Packing Size: 1100\*415\*230mm  Net Weight: 13.0KG  Gross Weight: 15.5KG Carton Packing: 1 set / ctn Container Loading:  20GP: 270 pcs  40GP: 560 pcs | **US$420.00** |

# RRMARK:

## 1: Above prices are based on EXW. Valid date to 31st Aug 2018. 2: 1~2 days for samples, 5~7 days for standard orders add 100% plus courier fee.

3: The solar controller and battery are built inside of light head.

4 : The controller needs extra 5.0USD, 10pcs of solar led street light need 1pc controller 5: Lighting mode can be changed by remote controller.