


|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | |  | | | | |
|  | | | | |
| **QUOTATION** | | | | | | |
|  | |  | |  | |  |
| E-mail | | [sales@asiandragonintl.com](mailto:sales@asiandragonintl.com) | |  | |  |
|  | |  | |  | |  |
|  | |  | | Quotation date  (valid time: 15 days) | | 2018.7.25 |
| **Project :Prefab House**  (HS code:9406900090 ;Picture just for reference ) | | | | | | |
|  | | | | | | |
| **House cost** | | | | | | |
| Item | Dimension | Area(㎡) | FOB Huangpu Price (/㎡) | Single Building Price ($) | Quantity(set) | Total price($) |
| House | 7.5 \*5.5 \*3m | 45.75 | $225.30 | $10,307.48 | 1 | $12,990.00 |
| Total Price | | | | | | $12,990.00 |
| The above is FOB Price | | | | | | |
| The price includes all the material show of the quotation. | | | | | | |



|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Remark** | | **Delivery Time:** 15 days after received 50% deposit, need final confirmation | | |
| **Payment:** T/T 50% as deposit, 50% balance before loading from factory | | |
| Loading: 1 x 20GP shipping containers. need final confirmation. | | |
| **Installation** | | 1. We can give you the processing drawing to guide the installation. 2. We can send our skill worker to your country to guide work,you need to provide return air tickets; visa cost,accommodation ,salary USD120/day.need to final confirmation | | |
| **Main Material Lists** | | | | |
| No. | Component | Materials  **(need to final confirmation ,according to design)** | Thickness (mm) | Photo |
| **Steel Structure** | | | | |
| 1 | Pillar | 100 \* 100mm square tube | 3mm |  |
| 2 | Ring Beam | 80\*80mm square tube | 2mm |  |
| 3 | Roof Purlin | 40\*80mm square tube | 1.8mm |  |
| 4 | Herringbone Beam | 8#C Steel | 1.8mm |  |
| **Wall Panel & Roof panel** | | | | |
| 5 | Wall Panel | EPS Sandwich Panel | 50\*950mm |  |



|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 6 | Partition Wall Panel | EPS Sandwich Panel | 50\*950mm |  |
| 7 | Roof Panel | EPS Sandwich Panel | 50\*950mm |  |
| 8 | Roof Tile | Asphalt Shingle | 3mm |  |
| **Decoration Ceiling & Wall Panel** | | | | |
| 9 | Ceiling Decoration | PVC ceiling board | 10mm | |
| 10 | Exterior Wall Decoration | PU decoration board | 16mm | |
| 11 | Interior Wall Decoration | Decoration Wall Panel | 300\*3000mm | |
| 12 | Floor Decoration | Ceramic Tile | 6mm | |
| 13 | Electric &water System | pipe,tap, wire,switch, socket, lamp |  | |
| **Window & Door** | | | | |
| 11 | Door | Alluminum Alloy Door | 800\*2000mm | |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 12 | Window | Aluminum Alloy Window | | 1000\*1200mm | |
| **Accessories** | | | | | |
| 13 | Accessories | screw,rivet,bolt and sealant etc | | |  |
| **Exported Countries** | | | | | |
| **Asia** : Korea，India ,Malaysia ,Thailand,Kuwait, Jordan ,Indonesia,Qatar,Oman,Philippines | | | **Europe:** Spain,England | | |
| **Africa:** Cameroon, mozambique, Mauritius,Ethiopia Angola,South Africa,Djibouti,Congo | | | **South America:** Trinidad andTobago,Chile, Brazil,Colombia,Bolivia,Suriname,Uruguay, venezuela | | |
| Oceania:Australia ，Kiribati | | |  | | |
| **Technical Parameter** | | | | | |
| No | Project Name | Value | No | Project Name | Value |
| 1 | Roof load | ≧65kilograms/m2 | 5 | Wall deformation | ≦65kilograms/m2 |
| 2 | Flooring load | ≧150kilograms/m2 | 6 | Seismic grade | 7-magnitude |
| 3 | Aisle load | ≧200kilograms/m2 | 7 | Wind loading | ≧100km/h |
| 4 | Wall side stress | ≧80kilograms/m2 | 8 | Fire proof | B1 grade |