

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | |  | | | |
|  | | | |
| **QUOTATION** | | | | | |
|  | |  | Contact person | | Myla Baracina |
|  | |  | E-mail | | [sales@asiandragonintl.com](mailto:sales@asiandragonintl.com) |
|  | |  |  | |  |
|  | |  | Quotation date (valid time:20 days) | | 2018.3.19 |
| **Project : Container House**  (HS code:9406900090 ;Picture just for reference ) | | | | | |
|  | | | | | |
| **Container House Cost** | | | | | |
| No. | Item | Dimension | **FOB H**uangpu USD$/set | Quantity | Total price |
| 1 | Container House | 11.8\*2.5\*2.6m | $7,300.00 | 1 | $7,300.00 |
| Total Price | | | | | $7,300.00 |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| FOB Huangpu Price include the house price, towing fee and custom fee, do not include other costs. | | | | |
| Remark | | **delivery time:** 30 days after received 30% deposit | | |
| **Payment:** T/T 50% as deposit, 50% balance before loading from factory | | |
| **Loading:** Need final confirmation | | |
| Installation | | 1. We can give you the processing drawing to guide the installation. 2. We can send our skill worker to your country to guide work, you need to provide return air tickets; visa cost, accommodation ,salary USD100/day.need to final confirmation | | |
| **Main Material Lists** | | | | |
| No. | Component | Materials  **(need to final confirmation ,according to design)** | Thickness (mm) | Photo |
| **Steel Structure** | | | | |
| 1 | Pillar | 100\*100mm Square tube | 3mm |  |
| 2 | Roof Ring Beam | 100\*100mm Square tube | 3mm |  |
| 3 | Ground Ring Beam | 100\*100mm Square tube | 3mm |  |
| 4 | Purlin | 8#C section steel | 1.7mm |  |
| **Wall Panel** | | | | |
| 5 | Wall Panel | Glass Wool Sandwich Panel | 50\*950\*0.326mm | |

|  |  |  |  |
| --- | --- | --- | --- |
| 6 | Partition Wall Panel | Glass Wool Sandwich Panel | 50\*950\*0.326mm |
| 7 | Roof Tile | Glass Wool Sandwich Panel | 50\*950\*0.326mm |
| **Floor & Ceiling** | | | |
| 8 | Floor | Fiber Cement Board | 15mm |
| 9 | Interior Floor Decoration | Ceramic | 6mm |
| 10 | Exterior Floor Decoration | Wood Plastic Floor Panel | 15mm |
| 11 | Ceiling Decoration | PVC Ceiling | 7mm |
| 12 | Interior Decoration Wall Panel | Decoration Panel | 10mm |
| 13 | Exterior Decoration Wall Panel | PU decoration board | 3080 \*380 \*16mm |
| **Window & Door** | | | |



|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 14 | Door | Aluminum Sliding Door | | 1600\*2000mm | |
| 15 | Window | Aluminum Sliding Window | | 1000\*1200mm | |
| 16 | Toilet Window | PVC Louver | | 800\*600mm | |
| **Accessories** | | | | | |
| 17 | Electric  &water system | pipe,tap, wire,switch, socket, lamp | | |  |
| 18 | Accessories | screw,rivet,bolt and sealant etc | | |  |
| **Exported Countries** | | | | | |
| **Asia** : Korea，India ,malaysia ,Thailad,Kuwait, Jordan ,Indonesia,Qatar,Oman,Philippines | | | **Europe:** Spain,England | | |
| **Africa:** Cameroon, mozambique, Mauritius, Angola,South Africa,Djibouti,Congo | | | **South America:** Trinidad andTobago,Chile, Brazil,Colombia,Bolivia,Suriname,Uruguay, venezuela | | |
| **Oceania:** Australia ，Kiribati | | |  | | |
| **Technical Parameter** | | | | | |
| No | Project Name | Value | No | Project Name | Value |
| 1 | Roof load | ≧65kilograms/m2 | 5 | Wall deformation | ≦65kilograms/m2 |
| 2 | Flooring load | ≧150kilograms/m2 | 6 | Seismic grade | 7-magnitude |
| 3 | Aisle load | ≧200kilograms/m2 | 7 | Wind loading | ≧100km/h |
| 4 | Wall side stress | ≧80kilograms/m2 | 8 | Fire proof | B1 grade |