

**Quotation for container house**

**the advantage of our company and folding container house is as follows**

1. modular house manufacture with CE and ISO certificate, with professional QC and after sale team to ensure the quality
2. fast installation, can be installed in 10 minutes
3. save storage space, if you don't need to use it, can fold it .it can be unfolded and folded more than 200 times
4. competitive price with good quality: we lower the price without lower the quality to give distributor more profit to do bigger business together
5. galvanized frame+painting,hard to rust. wall and roof with 50mm eps insulation
6. modular design, stacked 2 levels
7. easy to load and unload in container, because will add wheels on bottom.one 40HC container can load 10 units

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | | | | | |
| **No** | **item** | **specification** | **picture** | **unit price** | **options** |
| 1 | folding container house | Size:L5800mm\*W2480mm\*H2 470mm(folding size 5800mm\*2485mm\*460mm,inte rior size 5607mm\*2275mm\*2265mm) galvanized frame+powder coating  with one steel security door door two windows sliding window  50mm thickness sandwich panel for wall  steel sheet+50mm glass wool insulation+steel ceiling for roof 15mm MGO board for floor with electricity |  | USD 2099/UNIT EXW 1\*40HC  container can load 10 units(our frame is bigger and thicker,so we can only load 10 units  instead of 12 units) | change 50mm thickness insulation to 75mm plus USD 300  add pvc floor plus USD 200 |
| **remark** | | | | | |
| **payment terms:50% deposit by T/T,50% balance before shipment** | | | | | |
| **valid time:in 7 days** | | | | | |
| **lead time:30-40 days** | | | | | |

**the quotation is EXW price,fob charges for 1\*20ft container is USD 800,**

**fob charges for 1\*40HC container is USD 900**

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **material list for folding container house** | | | | | | | | | |
| **Project name:** | | | | | | | **Project No.:** | | |
| **Specification:** | | |  | **L5800mm\*W2480mm\*H2470mm** | | | **Area:** | **14.4** | **m2** |
| **NO** | **ITEM** | | **SPECIFICATION** | | **UNIT** | **QUANTI TY** |  |  | **PICTURE** |
| 1 |  | bottom main frame(other s is smaller size frame and thickness just 1mm) | | 200mm\*100mm\*2  .5mm L=5768mm galvanized steel+powder coating | pcs | 2.0 |  |  |  |
| 2 | 80\*80\*1.5mm L=2448mm not regular shape galvanized tube steel+powder coating | pcs | 2.0 |
| 3 | bottom secondary beam(other s frame thickness is just 1mm) | | 80\*80\*1.5mm L=2448mm not regular shape galvanized tube steel+powder coating | pcs | 9.0 |
| 4 | column(oth ers is smaller size frame and thickness just 1mm) | | 80\*80\*1.5mm L=975mm not regular shape galvanized tube steel+powder coating | pcs | 4.0 |
| 5 | 80\*80\*1.5mm L=935mm not regular shape galvanized tube steel+powder coating | pcs | 4.0 |
| 6 | Column | | 2.5mm thickness steel+powder coating L=1115mm | pcs | 2.0 |



frame

|  |
| --- |
| 7 |
| 8 |
| 9 |
| 10 |
| 11 |
| 12 |
| 13 |
| 14 |
| 15 |



US$2,499 US$2,499



|  |  |  |  |
| --- | --- | --- | --- |
| baffle | 2.5mm thickness steel+powder coating L=1075mm | pcs | 2.0 |
| long side wall(others is smaller size frame and thickness just 1mm) | 80\*80\*1.6mm L=5768mm not regular shape galvanized tube steel+powder coating | pcs | 8.0 |
| short side wall(others is smaller size frame and thickness just 1mm) | 80\*80\*1.5mm L=2275mm not regular shape galvanized tube steel+powder coating | pcs | 4.0 |
| 80\*80\*1.5mm L=2150mm not regular shape galvanized tube steel+powder coating | pcs | 4.0 |
| top main beam(other s is smaller size frame and thickness just 1mm) | 80\*80\*1.6mm L=5768mm not regular shape galvanized tube steel+powder coating | pcs | 2.0 |
| 80\*80\*1.6mm L=2290mm not regular shape galvanized tube steel+powder coating | pcs | 2.0 |
| top secondary beam | galvanized tube steel+powder coatiing | set | 1.0 |
| lifting point top | 175\*115\*97\*8mm | pcs | 4.0 |
| lifting point bottom | 285\*115\*97\*8mm | pcs | 4.0 |

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 16 |  | hinge(other s hinge is not so much thickness is thinner) | | 2.5mm thickness | pcs | 34.0 |  |  |  |
| 17 | top(others top panel is 0.4mm,ceiling is cheaper ceiling) | | 0.5mm steel sheet+50mm glass wool insulation+0.3mm steel ceiling | | set | 1.0 |  |
| 18 | wall panel | | 50mm thickness sandwich panel | | set | 1.0 |  |
| 19 | floor board | | 15mm MGO board | | set | 1.0 |  |
| 20 | steel door(others door is cheaper quality door) | | one set steel security door size 930\*2030mm | | pcs | 1.0 |  |
| 21 | sliding window | | two sets sliding window size 970\*1100 | | pcs | 2.0 |  |
| 22 | **TOTAL** | | | **EXW** | | | | **US$2,499** | |



 





