|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **QUOTATION SHEET NO:NC20230426** | | | | | | |
| Project name: White Cabin | | | | Size: Long 7000mm Wide 2300mm High 2550mm | | |
| HS code:9406900090 | | | | Date:2023-04-26 | | |
|  | | | | | | |
| No  . | Item | Specification | Quantity | Picture | Unit price  （USD) | Total(USD） |
| 1 | White Apple Cabin  （Without  Electrical Systems） | 7000\*2300\*2550mm  empty inside without tempered glass | 2 |  | 11600 | 23200 |
| EXW Price: 23,200 USD (2 units) | | | | | | |
| 1 | | **50%TT down payment before production,50%TT balance payment before ship** | | | | |
| 2 | | Design drawings are for reference only | | | | |
| 3 | | one 40HQ can load 1 unit | | | | |
| 4 | | The price is only valid within 15 days. | | | | |
| 5 | | within 30 working days after the receipt of down payment | | | | |





|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Materials for standard unit container house** | | | | |
| **NO** | **Items** | **Materials** | **Descriptions** | **Image** |
| 1 | steel frame | Bottom Main Beam | 60x80x3 mm galvanized square tube |  |
| 2 | Bottom Cross Beam | 50x50x3 mm galvanized square tube |
| 3 | Bottom connection beam | 80\*40\*2mm steel tube |
| 4 | Column | 60x80x3mm galvanized square tubel |
| 5 | L type slot | 30\*30mm 65\*65mm galvanized steel |
| 6 | Roof | External | Thickness of 0.5mm Steel Plate |  |
| Insulation layer | Thickness of 50mm EPS sandwich panel Density 20kg/m³ |
| Interior | Thickness of 0.5mm Steel Plate |
| Ceiling | 0.3 mm steel ceiling |
| 7 | Wall Waterproof | External | 0.5 mm GI steel |  |
| Insulation layer | Thickness of 50mm EPS sandwich panel Density 20kg/m³ |
| Interior | 0.5 mm GI steel |
|  |  |  |  |  |





|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 8 | Floor Waterproof | Base flooring | Thickness of 16mm waterproof  （cement） Board | |  |
| **Auxiliary parts** | | | | | |
| 1 | Decoration Line | PVC decoration accessories | for ceiling edge, | |  |
| for floor edge, | |
| for roof joint corner | |
| for corner post, | |
| 2 | Glue | Because packing and transportation, Please use them yourselves after the installation | Brand New | Full Sets |  |
| 3 | Screw | Brand New | Flat head Drilling screw 4.8\*38 | |  |
| Hexagonal drilling screw 5.5\*65 | |
| outside hexagonal screw 12\*20 | |
| Blind nut 14 | |

|  |  |
| --- | --- |
| **QUOTATION SHEET NO:vk20231116** | |
| Project name: 2024 Space capsule | Size: Long 8800mm Wide 2800mm High 2500mm |
| HS code:9406900090 | Date:2023-11-16 |
|  | |



|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | |
| No  . | Item | Specification | Quantity | Picture | Unit price  （USD) | Total(USD） |
| 1 | Space capsule (Electrical  Systems） | 8800\*2800\*2500mm  empty inside | 1 |  | $37,250.00 | $37,250.00 |
| 2 | Wooden plastic terrace | galvanized steel and wpc materials 2000mm\*4400mm | 1 |  | $700.00 | $700.00 |
| 3 | Toilet | Toilet, water mark certificated | 1 |  | $110.00 | $110.00 |
| 4 |  | glass shower door | 1 |  | $450.00 | $450.00 |





|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 5 | Shower room | partition wall | 1 |  | $110.00 | $110.00 |
| 6 | With shower nozzle cold&hot head  tiles floor installed in advance | 1 |  | $420.00 | $420.00 |
| 7 | pre-installed water pipr | 1 |  | $110.00 | $110.00 |
| 8 | Hand basin | with mixer-tap | 1 |  | $110.00 | $110.00 |
| 9 | Floor | Laminate Flooring  （Two colors can be selected） | 1 |  | $320.00 | $320.00 |
|  | | | | | | |
| 1 | | **50%TT down payment before production,50%TT balance payment before ship** | | | | |
| 2 | | Design drawings are for reference only | | | | |
| 3 | | The price is only valid within 15 days. | | | | |
| 4 | | within 30 working days after the receipt of down payment | | | | |
| **Materials for standard unit container house** | | | | | | |
| **NO** | **Items** | **Materials** | **Descriptions** | | **Image** | |







|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1 | steel frame | Bottom Main Beam | 60x80x3 mm galvanized square tube |  |
| 2 | Bottom Cross Beam | 50x50x3 mm galvanized square tube |
| 3 | Bottom connection beam | 80\*40\*2mm steel tube |
| 4 | Column | 60x80x3mm galvanized square tubel |
| 5 | L type slot | 30\*30mm 65\*65mm galvanized steel |
| 6 | Roof | External | Thickness of 0.5mm Steel Plate |  |
| Insulation layer | Thickness of 50mm EPS sandwich panel Density 20kg/m³ |
| Interior | Thickness of 0.5mm Steel Plate |
| Ceiling | 0.3 mm steel ceiling |
| 7 | Wall Waterproof | External | 0.5 mm GI steel |  |
| Insulation layer | Thickness of 50mm EPS sandwich panel Density 20kg/m³ |
| Interior | 0.5 mm GI steel |
|  |  |  |  |  |





|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 8 | Floor Waterproof | Base flooring | Thickness of 16mm waterproof  （cement） Board+12mm laminated floor | |  |
| **Auxiliary parts** | | | | | |
| 1 | Decoration Line | PVC decoration accessories | for ceiling edge, | |  |
| for floor edge, | |
| for roof joint corner | |
| for corner post, | |
| 2 | Glue | Because packing and transportation, Please use them yourselves after the installation | Brand New | Full Sets |  |
| 3 | Screw | Brand New | Flat head Drilling screw 4.8\*38 | |  |
| Hexagonal drilling screw 5.5\*65 | |
| outside hexagonal screw 12\*20 | |
| Blind nut 14 | |
|  | | | | | |